(a) (b) (c)

(d) (e)

(f)

(g)

(h)

(i)

Color plate: Partial reconstructions with increasing number of wavelet coefficients.

(a) 5000 coefficients, 98.5% compression, (b) 10000 coeff., 97% comp., (c) 2000 coeff., 94% comp., (d) 70000 coeff., 79% comp., (e) 100000 coeff., 69% comp., (f) zoom from (d), (g) same as in (f) with edges, (h) zoom from (e), (i) same as in (h) with edges